*Integration,*

*Differentiation,*

*Diode Static Resistance,*

*Diode Dynamic Resistance, r’d*

*Shunt Peaking Optimal Flatness improvement factor* = 1.414

* Low-Pass
* High-Pass

*Switching Transistors:*

* &
* )

*555 timers (two diode circuit):*

* ,